Par Statistics
Total Non-vccgnd Signals=7382
Total Non-vccgnd Design Pins=19885
Total Non-vccgnd Conns=19885
Total Non-vccgnd Timing Constrained Conns=18790
Phase 1 CPU=8.6 sec
Phase 2 CPU=9.9 sec
Phase 3 CPU=23.7 sec
Phase 4 CPU=24.3 sec
Phase 5 CPU=44.3 sec
Phase 6 CPU=44.3 sec
Phase 7 CPU=44.3 sec
Phase 8 CPU=44.3 sec
Phase 9 CPU=45.2 sec
Phase 10 CPU=47.3 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=7.7
AvgWirelenPerPin Fanout 4=8.0
AvgWirelenPerPin Fanout 10=5.2
AvgWirelenPerPin Fanout 50=4.2
AvgWirelenPerPin Fanout 100=8.3
AvgWirelenPerPin Fanout 500=3.4
AvgWirelenPerPin Fanout 5000=5.6
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=24.5878