-- Copyright (C) 1988-2002 Altera Corporation
-- Any megafunction design, and related net list (encrypted or decrypted),
-- support information, device programming or simulation file, and any other
-- associated documentation or information provided by Altera or a partner
-- under Altera's Megafunction Partnership Program may be used only to
-- program PLD devices (but not masked PLD devices) from Altera.  Any other
-- use of such megafunction design, net list, support information, device
-- programming or simulation file, or any other related documentation or
-- information is prohibited for any other purpose, including, but not
-- limited to modification, reverse engineering, de-compiling, or use with
-- any other silicon devices, unless such use is explicitly licensed under
-- a separate agreement with Altera or a megafunction partner.  Title to
-- the intellectual property, including patents, copyrights, trademarks,
-- trade secrets, or maskworks, embodied in any such megafunction design,
-- net list, support information, device programming or simulation file, or
-- any other related documentation or information provided by Altera or a
-- megafunction partner, remains with Altera, the megafunction partner, or
-- their respective licensors.  No other licenses, including any licenses
-- needed under any third party's intellectual property, are provided herein.



N.C. = No Connect. This pin has no internal connection to the device.
VCCINT = Dedicated power pin, which MUST be connected to VCC (3.3 volts).
VCCIO = Dedicated power pin, which MUST be connected to VCC (3.3 volts).
GND = Dedicated ground pin or unused dedicated input, which MUST be connected to GND.
RESERVED = Unused I/O pin, which MUST be left unconnected.

----------------------------------------------------------------------------

CHIP "fcnt" ASSIGNED TO AN EPM3064ATC44-10
TDI                              : 1
Mode1                            : 2
Mode0                            : 3
GND                              : 4
QFin                             : 5
CpuClk                           : 6
TMS                              : 7
QFref                            : 8
VCCIO                            : 9
Mode2                            : 10
GND                              : 11
GateIn                           : 12
CalibIn                          : 13
nReset                           : 14
FSync                            : 15
GND                              : 16
VCCINT                           : 17
RESERVED                         : 18
RESERVED                         : 19
RESERVED                         : 20
RESERVED                         : 21
RESERVED                         : 22
RESERVED                         : 23
GND                              : 24
RESERVED                         : 25
TCK                              : 26
PulseOut                         : 27
RESERVED                         : 28
VCCIO                            : 29
GND                              : 30
RESERVED                         : 31
TDO                              : 32
PulseIn                          : 33
RESERVED                         : 34
RESERVED                         : 35
GND                              : 36
Fin                              : 37
GND                              : 38
GND                              : 39
Fref                             : 40
VCCINT                           : 41
RESERVED                         : 42
SData                            : 43
SClock                           : 44
